CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.4/conf/instr/spect/uxnmr.info
Date         : Mon Jun 19 14:21:29 2023
Release      : TopSpin 3.6.4
Installed in : /opt/topspin3.6.4
Host         : b750
OS           : CentOS Linux release 7.6.1810 (Core) 
CPU          : Intel(R) Xeon(R) CPU E5-1620 v3 @ 3.50GHz (8 cores at 1300 MHz with Hyperthreading)
User         : nmrsu (NMR Super User)
System       : Avance III 750 NMR spectrometer
1H-frequency : 750.20 MHz
Description  : Avance III
Configured in: b750:/opt/topspin3.6.4/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.90
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: with digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : 1

DRU1: AQS DRU-E Z102520/00754 ECL 04.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2
DRU2: AQS DRU-E Z102520/00758 ECL 04.00
- TCP/IP address = 149.236.99.88
- Firmware Version = 170619

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x52   0x3    AW  R  3.0 REC-1  AQS RXAD1000 Z102118/145 ECL 03.00
     3   0x34 0xc1   0x1        X  2.0 REF-1  REF-1000 Reference Board for AQS Receiver
     4   0x24 0x29   0x8    AE  S  2.0 SGU-1  AQS SGU/2 1000 Z103082/00293 ECL 02.00 FPGA-Vs=AF
     6   0x11 0x52   0x3    AW  R  3.0 REC-2  AQS RXAD1000 Z102118/141 ECL 03.00
     7   0x25 0x29   0x8    AE  S  2.0 SGU-2  AQS SGU/2 1000 Z103082/00244 ECL 02.00 FPGA-Vs=AF
     8   0x26 0x29   0x8    AE  S  2.0 SGU-3  AQS SGU/2 1000 Z103082/00277 ECL 02.00 FPGA-Vs=AF
     9   0x27 0x29   0x8    AE  S  2.0 SGU-4  AQS SGU/2 1000 Z103082/00255 ECL 02.00 FPGA-Vs=AF
    10   0x3c 0xc5     0        Y  1.0 ROUT-1 AQS Router 1/4
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xc6     0        B  1.1 AQS/2  AQS/2 chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: 1 AQS Router 1/4


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345094_0016 W1345094/0016 ECL 0:
- TCP/IP address = 149.236.99.252
- Firmware VS    = 20120627
- Amplifier      = BLA2X500 E 6-365MHZ: W1345094/0016 ECL 0
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0227 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V V-USB: W1522040/0364 ECL 1
BLA_W1345097_0033 W1345097/0033 ECL 0:
- TCP/IP address = 149.236.99.251
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ: W1345097/0033 ECL 0
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0200 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/0160 ECL 2
BLA_W1345090_0008 W1345090/0008 ECL 0:
- TCP/IP address = 149.236.99.250
- Firmware VS    = 20120627
- Amplifier      = BLAH300 E 700-900MHZ: W1345090/0008 ECL 0
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0365 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V V-USB: W1522040/0378 ECL 2

Gradient amplifiers at the spectrometer subnet:
----------------------------------------------
BGA1: BGA_W1213762_0045
- TCP/IP address   = 149.236.99.243
- Firmware version = 20080206
- Web version      = 1.1
- Current limits   = -10.0/X, -10.0/Y, -10.0/Z (in A)

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20210921
- SCB channels = 40
- Shim System = BOSS3-SB
- 2HTX Amplifier: not available
- Lock: installed

Cryo Controller CRCO: device connected to 149.236.99.90:/dev/tty01

MAS2 control unit: connected to 149.236.99.90:/dev/tty04
MAS2: device not yet configured
MAS1: device could not be configured

Eurotherm VTU: device connected to 149.236.99.90:/dev/tty05

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                PN=Z003464, SN=00027 from 20060727
    Module  2 : XBB31P 2HS
                PN=Z003508, SN=00026 from 20070118
    Module  3 : 2H
                PN=Z003475, SN=00021 from 20060913
    Module  4 : HPHP 19F/1H
                PN=Z003547, SN=00005 from 20061019
    Module  5 : 13C
                PN=Z003526, SN=00012 from 20120123
    Module  6 : 15N
                PN=Z003532, SN=00010 from 20060915
    Module  7 : XBB31P 2HS
                PN=Z003508, SN=00028 from 20071026



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected via DPP to GREAT 3-10 Gradient Amplifier Unit W1213762/0045

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0033 at TCP/IP 149.236.99.251)
SGU1 AUX  output -> TUNE signal input of HPPR
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0033 at TCP/IP 149.236.99.251)
SGU2 AUX  output -> input 2 of transmitter 1 (BLA2X500 E 6-365MHZ W1345094/0016 at TCP/IP 149.236.99.252)
SGU3 NORM output -> input 1 of transmitter 1 (BLA2X500 E 6-365MHZ W1345094/0016 at TCP/IP 149.236.99.252)
SGU3 AUX  output -> input 2 of transmitter 3 (BLAH300 E 700-900MHZ W1345090/0008 at TCP/IP 149.236.99.250)
SGU4 NORM output -> input 1 of transmitter 3 (BLAH300 E 700-900MHZ W1345090/0008 at TCP/IP 149.236.99.250)
SGU4 AUX  output -> input of AQS Router 1/4
AQS Router 1/4 output 1 -> input 3 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0033 at TCP/IP 149.236.99.251)
AQS Router 1/4 output 2 -> input 3 of transmitter 1 (BLA2X500 E 6-365MHZ W1345094/0016 at TCP/IP 149.236.99.252)
AQS Router 1/4 output 3 -> input 3 of transmitter 3 (BLAH300 E 700-900MHZ W1345090/0008 at TCP/IP 149.236.99.250)
AQS Router 1/4 output 4 -> input 4 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0033 at TCP/IP 149.236.99.251)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLA2X500 E 6-365MHZ W1345094/0016 at TCP/IP 149.236.99.252:
- amplifier X-500W uses blanking 3
- amplifier X-500W uses blanking 4

transmitter 2 = BLAXH2H500/100/250 E 700-900MHZ W1345097/0033 at TCP/IP 149.236.99.251:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W needs no blanking

transmitter 3 = BLAH300 E 700-900MHZ W1345090/0008 at TCP/IP 149.236.99.250:
- amplifier 1H-300W uses blanking 5
- amplifier 1H-50W uses blanking 5


